This is probably the top break down, but also the easiest going get going again.

It ususally begins to show it's face by occasionally losing all power temorarily when the handlebars are turned to the extremes.

Not long after that the solder underneath the key will fail and all power will be lost.